**Lu Lab Incubator Monitor**

To Do:

* Add analog inputs w/ appropriate mapping
* Add SD data logging
* Make analog plugs for recorder input
* Make plugs for alarm inputs
* Use internal 1.1V AREF / Map analog values appropriately